BATTERY RECHARGING [L8, LF]

id0117a6800700

  Warning
  • Keep all flames away from the battery, otherwise evaporated gas from the battery fluid may catch fire, and cause serious injury.
  • Remove the battery filler caps when recharging to prevent battery deformation or damage.

  Caution
  • Do not quick charge for more than 30 min. It will damage the battery.

1. Remove the battery and then place it in a pan of water.

amxzzw00001986

2. Remove the battery filler caps.

3. Connect a battery charger to the battery and adjust the charging current as follows.

  Battery slow charge current

  46B24L (36 A·h/5HR, 45 A·h/20HR): 3.5—4.5 A

  Battery quick charge current [30 min]

  46B24L (36 A·h/5HR, 45 A·h/20HR): 25 A

4. After the battery is recharged, verify that the voltage is within the specification and remains at the same value for 1 h or more after the recharging has been completed.

  • If not within the specification, replace the battery.

  Standard voltage

  12.4 V or more