POWER OUTER MIRROR REMOVAL/INSTALLATION

id091200420800

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

4. Remove the door speaker. (See DOOR SPEAKER REMOVAL/INSTALLATION.)

5. Remove the door module panel.

6. Remove clips.

e5u912zw5057

7. Rotate the power outer mirror in the direction shown by the arrow.

amxzzw00000755

8. Remove the bolt.

amxzzw00001916

9. Rotate the power outer mirror in the direction shown by the arrow.

amxzzw00000756

10. Remove the bolt and the power outer mirror.

amxzzw00001917

11. Install in the reverse order of removal.