DOOR REMOVAL/INSTALLATION

id091100620500

1. Disconnect the negative battery cable.(See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove in the order indicated in the table.

amxzzw00000216

1 | Connector (See Connector Removal Note.)
2 | Bolt A
3 | Bolt B
4 | Door

3. Install in the reverse order of removal.

4. Adjust the door. (See DOOR ADJUSTMENT.)

Connector Removal Note

1. Pull down the lever in the direction indicated by the arrow and disconnect the connector.

amxzzw00000167