FRONT UPPER ARM REMOVAL/INSTALLATION

id021300801900

  Caution
  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the wiring harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled while servicing the vehicle.

1. For 6MT vehicles, perform the following procedures.

  (1) Disconnect the purge solenoid valve connector wiring harness from the bracket.

  (2) Remove the bracket from the air intake hose and move the purge solenoid valve component out of the way. (See PURGE SOLENOID VALVE REMOVAL/INSTALLATION [L8, LF].)

  (3) Remove the following parts as a single unit. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L8, LF].)
    ― Air intake hose
    ― Resonance chamber No. 2
    ― Resonance duct No. 1
    ― Resonance duct No. 2

2. Remove the front suspension tower bar. (See FRONT SUSPENSION TOWER BAR REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

5. Inspect the front wheel alignment and adjust it if necessary. (See FRONT WHEEL ALIGNMENT.)

e5u213zw5004

1 | Brake hose bracket
2 | Front upper arm ball joint (See Front Upper Arm Ball Joint Removal Note.)
3 | Front shock absorber, coil spring and front upper arm (See Front Shock Absorber, Coil Spring And Front Upper Arm Removal Note.)
4 | Front upper arm (See Front Upper Arm Removal Note.)

Front Upper Arm Ball Joint Removal Note

1. Remove the front upper arm ball joint from the steering knuckle using the SST.

amxzzw00000052

Front Shock Absorber, Coil Spring And Front Upper Arm Removal Note

1. Loosen the shock absorber upper nuts.

2. Remove the front shock absorber lower bolt and nut.

Front Upper Arm Removal Note

1. Remove the front upper arm bolts.

2. Push down the front lower arm, and then remove the front upper arm from the gap between the shock absorber lower end and the front lower arm.