SIDE SILL REINFORCEMENT (FRONT) REMOVAL [PANEL REPLACEMENT]

id098008616200

1. Rough cut and remove the damaged part of the side sill reinforcement (front).

  Caution
  • During rough cutting, be careful not to damage the front pillar reinforcement indicated by dotted lines in the figure.

  Note
  • If the nut plate is not damaged, do not dispose of it, as it can be reinstalled. If it is damaged considerably, replace it with a new one.

amxzzb00000022