DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

id081000801300

  Warning
  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)

1. Turn the ignition switch to the LOCK position.

2. Remove the battery cover.

3. Disconnect the negative battery cable and wait for 1 min or more. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

4. Remove the covers.

amxzzw00001787

5. Remove the bolts.

6. Using a flathead screwdriver, lift the locking device carefully, however do not remove it.

amxzzw00001788

7. Disconnect the air bag module connector.

8. Disconnect the horn switch connector.

9. Remove the driver-side air bag module.

10. Install in the reverse order of removal.

11. Turn the ignition switch to the ON position.

12. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system. (See FOREWORD [AIR BAG SYSTEM].)