MASS AIR FLOW (MAF)/INTAKE AIR TEMPERATURE (IAT) SENSOR REMOVAL/INSTALLATION [L8, LF]

id0140i7805500

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect MAF/IAT sensor connector.

4. Remove the MAF/IAT sensor.

e5u140zw5302

5. Install in the reverse order of removal.

  MAF/IAT sensor tightening torque

  0.55—0.82 N·m {5.7—8.3 kgf·cm, 4.9—7.2 in·lbf}