NO.4 CANNOT TUNE (SEEK DOES NOT STOP) [RADIO]

id0903e3804600

4 | Cannot tune (seek does not stop)
--- | ---
Possible DTC | 09:Er20, 09:Er22
POSSIBLE CAUSE | • Center panel malfunction • Electronic jamming from outside, or inferior condition of broadcasting station radio wave • Antenna plug poor connection • Antenna feeder malfunction • Audio unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect if feel of SEEK switch is normal when switch is pushed and released. • Is it okay? | Yes | Go to the next step.
No | Perform confirmation step 1: center panel switch confirmation. Replace center panel if necessary.
2 | • Inspect indication of LCD. • Is frequency indication increased or decreased when SEEK switch is pushed? | Yes | Go to the next step.
No | Perform confirmation step 1: center panel switch confirmation. Replace center panel if necessary.
3 | • Manually tune to local broadcasting station and check reception condition. • Is reception okay? | Yes | Go to the step 6.
No | Go to the next step.
4 | • Inspect antenna plug connection condition. • Is connection okay? | Yes | Go to the next step.
No | Insert antenna plug securely.
5 | • Turn ignition switch to LOCK position. • Measure continuity between antenna feeder axis and ground. • Is there any continuity? | Yes | Replace antenna feeder.
No | Go to the next step.
6 | • Check if number of broadcasting stations changes depending on time and place. • Does it change? | Yes | The system is normal. (Explain to customer that SEEK sometimes does not stop depending on signal reception condition) Note • Signals tend to reach longer distances in the night. It is conspicuous in AM signals, several audio functions may stop due to foreign broadcasting station or noise. Though the audio system restrains sensitivity of SEEK and SCAN functions in the night, the audio system may select other than desired broadcasting station when signals are considerably strong. This function is linked to the parking light. When the parking light or headlight is turned on, SEEK and SCAN may not function for weak signals.
No | Replace audio unit. (See CENTER PANEL UNIT REMOVAL/INSTALLATION.) (See CENTER PANEL UNIT DISASSEMBLY/ASSEMBLY.)