A/C COMPRESSOR CONTROL OPERATION [FULL-AUTO AIR CONDITIONER]

id0740a1103200

A/C Compressor Automatic Control

• If the evaporator temperature reaches the specification, the A/C signal (magnetic clutch) is turned on/off to protect the A/C compressor.

amxzzn00000357

Correction

Defroster correction
• When the mode dial is turned to defroster, the A/C turns on to improve defrosting.

A/C Compressor Manual Control

• A/C on or off mode is selected by operating the A/C switch.