CRUISE CONTROL SWITCH INSPECTION [L8, LF]

id0120b1800100

1. Remove the battery cover. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove the driver‐side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

4. Disconnect the clock spring (cruise control switch-side) connector.

5. Inspect for resistance and continuity between terminals B—C (part-side) using a tester.

  • If not as specified, replace the cruise control switch. (See AUDIO CONTROL SWITCH REMOVAL/INSTALLATION.)

Switch Condition | Resistance (Ohm) | System Wiring Diagram
--- | --- | ---
ON OFF switch pressed | Continuity |
CANCEL switch pressed | Approx. 120
SET/– switch pressed | Approx. 680
RES/+ switch pressed | Approx. 2.200
No switch pressed | No continuity