STEERING SPECIFICATIONS

id060000100300

Item | Specification
--- | ---
Steering wheel | Outer diameter | (mm {in}) | 370 {14.6}
Lock-to-lock | (turns) | 2.6
Steering gear and linkage | Type | Rack-and-pinion
Rack stroke | (mm {in}) | 156.4 {6.157}
Steering column and shaft | Shaft type | Collapsible
Joint type | 2-cross joint
Amount of tilt | (mm {in}) | 32 {1.3}
Power steering system | Power assist type | Engine speed sensing
Power steering fluid | Type | ATF M-III or equivalent (e.g. Dexron®II)
Fluid capacity*1 (approximate quantity) | L.H.D.: 1.19 {1.26, 1.05} R.H.D.: 1.17 {1.24, 1.03}
(L {US qt, Imp qt})

*1 :When fluid reservoir is at maximum volume.