TURBINE SENSOR REMOVAL/INSTALLATION [SJ6A-EL]

id051311252000

  Caution
  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.
  • Do not damage the turbine sensor.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Disconnect the turbine sensor connector.

4. Remove the turbine sensor.

e5u513zw5070

5. Install the turbine sensor.

  Tightening torque

  3.9—6.9 N·m {40—70 kgf·cm, 35—60 in·lbf}

6. Connect the turbine sensor connector.

7. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

8. Install the battery cover.