STEERING GEAR AND LINKAGE REMOVAL/INSTALLATION

id061400800900

  Caution
  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (axle side) and fix it to an appropriate place where the sensor will not be pulled by mistake while servicing the vehicle.

1. Remove the ABS wheel-speed sensor. (See FRONT ABS WHEEL-SPEED SENSOR REMOVAL/INSTALLATION.)

2. Remove the splash shield A. (See SPLASH SHIELD REMOVAL/INSTALLATION.)

3. Remove the front under cover. (See FRONT UNDER COVER REMOVAL/INSTALLATION.)

4. Remove the front stabilizer. (See FRONT STABILIZER REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

7. After installation, adjust front wheel alignment. (See FRONT WHEEL ALIGNMENT.)

amxzzw00001468

1 | Bolt (intermediate shaft) (See Bolt (Intermediate Shaft) Removal Note.) (See Bolt (Intermediate Shaft) Installation Note.)
2 | Cotter pin
3 | Nuts (tie-rod end ball joint)
4 | Tie-rod end ball joint (See Tie-rod End Ball Joint Removal Note.)
5 | Radiator lower mount rubber bracket
6 | Pressure pipe
7 | Return hose
8 | Steering gear and linkage (See Steering Gear and Linkage Removal Note.) (See Steering Gear and Linkage Installation Note.)
9 | Return pipe

Bolt (Intermediate Shaft) Removal Note

1. Mark the pinion shaft and gear housing for proper installation.

amxzzw00001469

Tie-rod End Ball Joint Removal Note

1. Remove the tie-rod nut.

2. Separate the tie-rod end from the steering knuckle using the SSTs.

amxzzw00001470

Steering Gear and Linkage Removal Note

1. Remove the steering gear and linkage by pulling it from the right side.

Steering Gear and Linkage Installation Note

1. Tighten bolts loosely.

2. Assemble the mounting bracket with the mark on the bracket facing the vehicle rear.

amxzzw00001471

3. Tighten the mounting bracket bolts to the specified torque in the order shown.

amxzzw00001472

  Tightening torque

  74.4—104.8 N·m {7.587—10.68 kgf·m, 54.88—77.29 ft·lbf}

Bolt (Intermediate Shaft) Installation Note

1. Align the marks and install the intermediate shaft and bolt.