POWER STEERING PRESSURE (PSP) SWITCH INSPECTION [L8, LF]

id0140i7803100

1. Inspect the following items:

  • Power steering fluid amount (See POWER STEERING FLUID INSPECTION.)
  • Power steering-related inspection (See STEERING LOCATION INDEX.)

2. Disconnect the PSP switch connector.

3. Start the engine.

4. Verify that the continuity between PSP switch terminal A and body ground is as indicated in the table.

  • If not as indicated in the table, replace the PSP switch. (See POWER STEERING OIL PUMP DISASSEMBLY/ASSEMBLY.)

Specification

Measured condition | Continuity
--- | ---
Steering wheel in straight ahead position | No continuity
While turning sttering wheel | Continuity detected