DTC B1193:00 [ACTIVE BONNET]

id0802f1822000

DESCRIPTION | Recording of active bonnet control module collision data
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the diagnostic procedure. • After the active bonnet actuator has operated, the active bonnet control module completes recording of collision data
POSSIBLE CAUSE | • Active bonnet actuator operation • Active bonnet control module malfunction

Diagnostic Procedure

Action
Replace the active bonnet control module. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.)