DTC B2143

id020200800400

DESCRIPTION | ID registration failure
--- | ---
DETECTION CONDITION | • Two or more codes are overlapping.
POSSIBLE CAUSE | • ID registration procedure has not been performed properly.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY PROGRAMMED ID • Turn the ignition switch off. • Connect the M-MDS to the DLC-2. • Perform the PID/Data Monitor and Record Procedure and select the following PIDs using the M-MDS: (See TIRE PRESSURE MONITORING SYSTEM (TPMS) ON-BOARD DIAGNOSIS.) ― ID_WU1 ― ID_WU2 ― ID_WU3 ― ID_WU4 • Turn the ignition switch to the ON position. • Is the same code in the output ID? | Yes | Perform the instrument cluster configuration, register the wheel unit ID, and then go to the next step. (See INSTRUMENT CLUSTER CONFIGURATION.) (See WHEEL UNIT ID REGISTRATION.)
No | Go to the next step.
2 | VERIFY TROUBLESHOOTING COMPLETED • Perform the Clearing DTCs Procedure. (See TIRE PRESSURE MONITORING SYSTEM (TPMS) ON-BOARD DIAGNOSIS.) • Drive the vehicle at a speed of 25 km/h {15.5 mph} or more for 10 min or more. • Perform the Reading DTCs Procedure. (See TIRE PRESSURE MONITORING SYSTEM (TPMS) ON-BOARD DIAGNOSIS.) • Is the same DTC present? | Yes | Repeat the inspection from Step 1. If the malfunction recurs: • Replace the instrument cluster and/or wheel unit, then go to the next step. (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.) (See WHEEL UNIT REMOVAL/INSTALLATION.)
No | Go to the next step.
3 | VERIFY AFTER REPAIR PROCEDURE • Are any DTCs present? | Yes | Go to the applicable DTC inspection. (See TIRE PRESSURE MONITORING SYSTEM (TPMS) ON-BOARD DIAGNOSIS.)
No | DTC troubleshooting completed.