POWER OUTER MIRROR DISASSEMBLY/ASSEMBLY

id091200807300

1. Remove the outer mirror glass. (See Outer Mirror Glass Disassembly Note.) (See Outer Mirror Glass Assembly Note.)

amxzzw00000722

2. Assemble in the reverse order of disassembly.

Outer Mirror Glass Disassembly Note

1. Press area A of the outer mirror glass so that area B moves outward.

e5u912zw5018

2. Detach pin A while lifting up the inside of the outer mirror glass holder.

amxzzw00000723

3. Pull out the outer mirror glass holder and detach pins B.

4. Disconnect the connector. (vehicles with heated outer mirrors)

5. Remove the outer mirror glass holder and the outer mirror glass as a single unit.

Outer Mirror Glass Assembly Note

1. Connect the connector. (vehicles with heated outer mirrors)

2. Press area A of the mirror glass into the base to attach pin A.

amxzzw00000723

3. Press areas B of the outer mirror glass into the base to attach pins B.