FOREWORD [SJ6A-EL]

id050307800200

• When the customer reports a vehicle malfunction, inspect the malfunction indicator lamp (MIL) indication, AT warning indicator light flash, and diagnostic trouble code (DTC), then diagnose the malfunction according to following flowchart:

  ― If a DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [SJ6A-EL].)
  ― If a DTC does not exist, the MIL does not illuminate and the AT warning indicator light illuminate, diagnose the applicable symptom troubleshooting. (See SYMPTOM TROUBLESHOOTING ITEM TABLE [SJ6A-EL].)

  Note
  • If a tire of a different diameter from the standard tire is installed, the TCM determines that the driving mode is the AAS mode, and may change to a different shift timing from the normal timing.

amxuuw00001550

*: Malfunction Indicator Lamp (MIL), AT warning light.