FRONT FRAME COMPONENT (FRONT) INSTALLATION [PANEL REPLACEMENT]

id098008606400

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for plug welds before installing new parts.

3. After temporarily installing new parts, make sure the related parts fit properly.

  Caution
  • Plug weld the 2 weld locations indicated by (A) together with the front side frame rear reinforcement.

d5u0980b142

d5u0980b143