VALVE GUIDE REPLACEMENT

id011000501200

Valve Guide Removal

1. Remove the valve guide from the combustion chamber side using the SST.

belbze00000121

Valve Guide Installation

1. Assemble the SSTs so that depth L is as specified.

belbze00000122

  Depth L:

  12.2—12.8 mm {0.481—0.503 in}

2. Tap the valve guide in from the cam side using the SSTs assembled in Step 1.

belbze00000123

3. Verify that the valve guide protrusion height (dimension A) is within the specification using the vernier caliper.

belbze00000124

  Standard height:

  12.2—12.8 mm {0.481—0.503 in}