REAR BUMPER REINFORCEMENT REMOVAL/INSTALLATION

id091000800900

1. Disconnect the negative battery cable. (SeeBATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (2) Partition board (See PARTITION BOARD REMOVAL/INSTALLATION.)

  (3) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Rear combination lights (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

  (5) Rear bumper (See REAR BUMPER REMOVAL/INSTALLATION.)

3. Remove the nuts, then remove the rear bumper reinforcement.

e5u910zw1022

4. Install in the reverse order of removal.