GENERAL PRECAUTION (STEERING)

id061000800300

Wheels and Tire Installation

1. When installing the wheels and tires, tighten the wheel nuts in a criss-cross pattern to the following tightening torque.

  Tightening torque

  88—118 N·m {9.00—12.0 kgf·m, 65.0—87.0 ft·lbf}

Connector Disconnection

1. Disconnect the negative battery cable before performing any work that requires handling of connectors. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

Power Steering Components Removal/Installation

1. If any power steering fluid line has been disconnected anytime during the procedure, add ATF M-III or equivalent (e.g. Dexron®II), bleed the fluid lines, and inspect for leakage after the procedure has been completed.