POWER RETRACTABLE HARDTOP SWITCH CONSTRUCTION/OPERATION

id091600102000

• The power retractable hardtop switch is integrated with the hazard warning switch.
• The operational switch operates at the point the switch has been continuously pressed on for 100 ms.
• Depending on the power retractable hardtop position and operation conditions, the operation switch input reception is restricted as follows:

Power retractable hardtop position | Power retractable hardtop open switch input | Power retractable hardtop close switch input | Power retractable hardtop operation after switch determined to be on/off | Restriction
--- | --- | --- | --- | ---
Power retractable hardtop position | Power retractable hardtop operation
Full open | Stopped | ON | OFF | Stop | power retractable hardtop open switch inoperative
Full closed | Stopped | OFF | On operation | Stop | power retractable hardtop close switch inoperative
All positions | Stopped | ON at the same time | ON at the same time | Stop | power retractable hardtop open and close switch inoperative
Full open | Stopped | During ON | Operates afterward | Stop | power retractable hardtop close switch inoperative
Full closed | Stopped | Operates afterward | During ON | Stop | power retractable hardtop open switch inoperative
Except fully open | During open operation | During ON | On operation afterward | operations stop | power retractable hardtop open and close switch inoperative
Except fully closed | During close operation | On operation afterward | During ON | operations stop | power retractable hardtop open and close switch inoperative

• Once the operation switch has operated, the next operation switch does not operate unless an off-operation for the switch operation is detected.