TRUNK LID OPENER RELAY REMOVAL/INSTALLATION

id092100801900

  Note
  • Depending on the period of manufacture, the trunk lid opener relay and rear fog relay positions may be switched. When performing removal/installation and inspection, make determinations based on wiring color.
    ― Terminal A: violet
    ― Terminal C: blue/red
    ― Terminal D: blue
    ― Terminal E: blue/red (without power retractable hardtop), white/red (with power retractable hardtop)

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the trunk end trim. (See TRUNK END TRIM REMOVAL/INSTALLATION.)

4. Remove the trunk lid opener relay.

amxzzw00002150

5. Install in the reverse order of removal.