POWER WINDOW REGULATOR DISASSEMBLY/ASSEMBLY

id091200812900

1. Remove in the order indicated in the table.

amxzzw00000726

1 | Cover (See Cover Disassembly Note.)
2 | Power window motor
3 | Frame

2. Assemble in the reverse order of disassembly.

  Note
  • When installing the power window motor, be careful that the cable does not become unwounded from the drum.

Cover Disassembly Note

1. Carefully bend away the crimp of the cover using long nose pliers.

e5u912zw5049