DOOR GLASS ADJUSTMENT

id091200813100

1. Fully close the door glass.

2. Remove the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the door module panel. (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

4. Connect the power window regulator connector.

5. Loosen the glass stopper installation bolts.

e5u912zw5059

6. Loosen the power window regulator and door glass tightening nuts.

7. Align the door glass with the rear edge of the front beltline molding lip.

  Note
  • The standard position for the rear edge of the cap is 1 mm from the rear edge of the door panel. If the standard position for the rear edge of the front beltline molding has deviated, align the rear edge of the door glass to the standard position for the rear edge position of the front beltline molding lip.

amxzzw00000727

8. Lightly tighten the power window regulator and door glass tightening nuts.

9. Adjust the clearance between the upper edge of the door glass and the door glass guide.

amxzzw00000728

mm {in}

Clearance | Standard | Minimum | Maximum
--- | --- | --- | ---
a | 1.0 {0.04} | 0 {0} | 1.5 {0.06}

10. Adjust the door glass position.

amxzzw00000729

11. Tighten the power window regulator and door glass tightening nuts.

e5u912zw5062

12. Tighten the bolts while pressing the glass stopper in the direction of the arrows.

e5u912zw5063

13. Verify that the door glass opens and closes smoothly.

14. Install the door module panel. (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

15. Install the door trim. (See DOOR TRIM REMOVAL/INSTALLATION.)

16. Close the door with the soft top closed and verify that the door glass opens and closes smoothly.