PARAMETER IDENTIFICATION (PID) DATA MONITORING FUNCTION [SJ6A-EL]

id050208100700

• The PID mode allows access to certain data values, analog and digital input and output, calculations and system state information.

Monitor Item Table

Display on the tester | Definition | Unit/Condition | TCM terminal
--- | --- | --- | ---
BOO TCM | Brake switch | On/Off | N/A
DTCCNT | DTC count (includes those needing no action) | N/A | N/A
DWN SW | Down switch | On/Off | 2F
ECT TCM | Engine coolant temperature | °C | N/A
FDPDTC | Freeze frame data | N/A | N/A
GEAR_RA | Gear ratio | N/A | N/A
GEAR_SEL | Calculated gear range in TCM | 1/2/3/4/5/6 | N/A
LPS | Line pressure control solenoid | A | 1E, 1R
MNL SW | M range switch | On/Off | 2G
OSS | Output shaft speed | RPM | 2C, 2D
PNP_TCM | Park/Neutral | Drive/Neutral | 2K, 2M, 2N, 2O
RPM TCM | Engine speed | RPM | N/A
SS SW- | Steering shift switch (shift down) | On/Off | 2AB, 2AF
SS SW+ | Steering shift switch (shift up) | On/Off | 2AB, 2AF
SSA | Shift solenoid A | On/Off | 1AF
SSB | Shift solenoid B | On/Off | 1AB
SSC | Shift solenoid C | On/Off | 1AA
SSD | Shift solenoid D | On/Off | 1S
SSE | Shift solenoid E | On/Off | 1V
SSF | Shift solenoid F | A | 1O, 1Z
SSG | Shift solenoid G | A | 1L, 1Y
TCCC | TCC control solenoid | A | 1D, 1Q
TFT | ATF temperature | °C | 1J, 1M
TFTV | ATF temperature signal voltage | V | 1J, 1M
THOP | Throttle position | % | N/A
TR | TR switch | R/N/D/P | 2K, 2M, 2N, 2O
TRD | TR switch [D range] | On/Off | 2K
TRR | TR switch [R position] | On/Off | 2M
TSS | Input/turbine speed sensor | RPM | 2A, 2B
UP SW | Up switch | On/Off | 2J
VPWR_TCM | Battery voltage | V | 1AD
VSS | Vehicle speed | KPH | 2C, 2D