BOLT INSPECTION

id011000503300

1. Measure the length of each bolt.

  • If it exceeds the specification, replace the bolt.

belbze00000219

  Bolt length (mm {in})

  Cylinder head bolt (With washer)
  Standard: 149.2—149.8 {5.875—5.897}
  Maximum: 150.5 {5.925}
  Cylinder head bolt (Without washer)
  Standard: 145.2—145.8 {5.72—5.74}
  Maximum: 146.5 {5.77}
  Connecting rod bolt
  Standard: 43.7—44.3 {1.73—1.74}
  Maximum: 45.0 {1.77}
  Main bearing cap bolt (Plastic region tightening bolt only)
  Standard: 110.0—110.6 {4.33—4.35}
  Maximum: 111.3 {4.38}