AudioPilot®2 MICROPHONE REMOVAL/INSTALLATION

id092000866300

  Note
  • AudioPilot® 2 is a registered trademark of Bose® Corporation.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove in the order indicated in the table.

amxzzw00001678

1 | Connector
2 | Screw
3 | AudioPilot® 2 microphone

4. Install in the reverse order of removal.