TRANSMISSION RANGE (TR) SWITCH ADJUSTMENT [SJ6A-EL]

id051311251600

  Caution
  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the tunnel member component.

4. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

5. Remove the insulator.

amxzzw00000191

6. Mark the manual shaft lever component as shown in the figure.

e5u513zw5007

7. Separate the manual shaft lever component from selector lever.

8. Disconnect the TR switch connector.

e5u513zw5006

9. Rotate the manual shaft to the N position.

  Caution
  • Do not use an impact wrench. Hold the manual shaft lever when removing the manual shaft nut, otherwise the transmission may be damaged.

10. Set the adjustable wrench as shown in the figure to hold the manual shaft lever.

amxzzw00000192

11. Remove the manual shaft nut.

12. Remove the washer and manual shaft lever component.

e5u513zw5009

13. Loosen the TR switch mounting bolts.

14. Temporarily install the TR switch mounting bolt.

  Caution
  • Improper adjustment of the TR switch will cause abnormal operation of the automatic transmission. Be sure to adjust the TR switch correctly.

15. Verify the TR switch reference line and the notch of the manual shaft are aligned.

e5u513zw5081

16. Tighten the TR switch mounting bolts.

  Tightening torque

  9.8—15.7 N·m {100—160 kgf·cm, 87—138 in·lbf}

17. Inspect for continuity between TR switch terminals E and H.

amxzzw00000193

18. Install the manual shaft lever component and washer.

  Caution
  • Do not use an impact wrench. Hold the manual shaft lever when tightening the manual shaft nut, otherwise the transmission may be damaged.

19. Set the adjustable wrench as shown in the figure to hold the manual shaft lever.

amxzzw00000194

20. Tighten the manual shaft nut using a torque wrench.

  Tightening torque

  14—18 N·m {1.5—1.8 kgf·m, 11—13 ft·lbf}

21. Shift the selector lever to P position.

22. Turn the manual shaft lever to P position.

23. Inspect TR switch continuity. (See TRANSMISSION RANGE (TR) SWITCH INSPECTION [SJ6A-EL].)

24. Connect the TR switch connector.

25. Align the mark of the manual shaft lever component as shown in the figure.

e5u513zw5007

26. Install the manual shaft lever component installation nut.

  Tightening torque

  10.8—14.7 N·m {111—149 kgf·cm, 96.4—129.3 in·lbf}

27. Install the insulator.

  Tightening torque

  8—11 N·m {82—112 kgf·cm, 72—97 in·lbf}

28. Install the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

29. Install the tunnel member component.

30. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

31. Install the battery cover.

32. Inspect TR switch operation. (See TRANSMISSION RANGE (TR) SWITCH INSPECTION [SJ6A-EL].)