TRUNK COMPARTMENT LIGHT BULB REMOVAL/INSTALLATION

id091800806200

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Slide the trunk component light in the direction of the arrow (1) in the figure, then pull it in the direction of the arrow (2).

amxzzw00001087

4. Remove the trunk compartment light.

5. Disconnect the trunk compartment light connector.

6. Remove the trunk compartment light bulb.

7. Install in the reverse order of removal.