NO.26 STARTER DOES NOT WORK [SJ6A-EL]

id050307803100

26 | Starter does not work
DESCRIPTION | • Starter does not work even when P or N position is selected.
POSSIBLE CAUSE | • Selector lever malfunction • Manual shaft malfunction • TR switch malfunction • TR switch mis-adjustment • Transmission operates in fail-safe function (Starter lock system related circuit open or short) • Immobilizer system operating or system malfunction.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Inspect the selector lever, TR switch and manual shaft positions. • Are these position normal? | Yes | Go to the next step.
No | Adjust or replace the suspect part position.
2 | • Inspect the TR switch. (See TRANSMISSION RANGE (TR) SWITCH INSPECTION [SJ6A-EL].) • Is the TR switch normal? | Yes | Perform the symptom troubleshooting “NO.3 WILL NOT CRANK”. (See NO.3 WILL NOT CRANK [L8, LF].)
No | Replace the TR switch. (See TRANSMISSION RANGE (TR) SWITCH REMOVAL/INSTALLATION [SJ6A-EL].)
3 | • Verify test results. ― If normal, return to the diagnostic index to service any additional symptoms. ― If malfunction remains, inspect the related Service Information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM. (See TCM REMOVAL/INSTALLATION [SJ6A-EL].)