DTC B1342 [DYNAMIC STABILITY CONTROL (DSC)]

id0402b2809000

DTC | B1342 | DSC HU/CM system
DETECTION CONDITION | • The DSC HU/CM on-board diagnostic function detects control module malfunction.
POSSIBLE CAUSE | • DSC HU/CM internal malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear the DTC from the memory. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) • Start the engine and drive the vehicle at 10 km/h {6.2 mph} or more. • Is the same DTC present? (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) | Yes | Replace the DSC HU/CM, then go to the next step. (See DSC HU/CM REMOVAL/INSTALLATION.)
No | Go to the next step.
2 | VERIFY AFTER REPAIR PROCEDURE • Are any other DTCs present? (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].) | Yes | Go to the applicable DTC inspection. (See ON-BOARD DIAGNOSIS [DYNAMIC STABILITY CONTROL (DSC)].)
No | DTC troubleshooting completed.