FRONT SHOCK ABSORBER INSPECTION

id021300104400

1. Remove the front shock absorber.

2. Inspect for damage and oil leakage.

3. Compress and extend the shock absorber piston rod at least three times at a steady speed. From the fourth compression stroke, verify that the operational force does not change and that there is no unusual noise.

  • If there is any malfunction, replace the shock absorber.