SAS CONTROL MODULE REMOVAL/INSTALLATION

id081000801400

  Warning
  • Handling the SAS control module improperly can accidentally deploy the air bag modules and pre-tensioner seat belt, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See AIR BAG SYSTEM SERVICE WARNINGS.) (See AIR BAG SYSTEM SERVICE CAUTIONS.)

  Caution
  • Handling the SAS control module improperly can accidentally deploy the air bag modules and pre-tensioner seat belt, which may seriously injure you. If configuration is not completed before removing the SAS control module, DTC B2477 will be displayed.

1. Perform SAS control module configuration when replacing it. (See SAS CONTROL MODULE CONFIGURATION.)

2. Turn the ignition switch to the LOCK position.

3. Remove the battery cover.

4. Disconnect the negative battery cable and wait for 1 min or more. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

5. Remove the console. (See CONSOLE REMOVAL/INSTALLATION.)

6. Remove the side wall. (See SIDE WALL REMOVAL/INSTALLATION.)

7. Remove the console panel. (See CONSOLE PANEL REMOVAL/INSTALLATION.)

8. Disconnect the connector

9. Remove the bolts.

amxzzw00001789

10. Remove the SAS control module.

11. Install in the reverse order of removal.

12. Turn the ignition switch to the ON position.

  • If the SAS control module is replaced, turn the ignition switch to the ON position for 20 s or more after completing the configuration.

13. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system. (See FLOWCHART [AIR BAG SYSTEM].)