DTC B1425:55 [ACTIVE BONNET]

id0802f1003300

DESCRIPTION | Active bonnet control module internal malfunction
--- | ---
DETECTION CONDITION | Warning • Detection conditions are for understanding the DTC outline before performing an inspection. Performing an inspection according to only the detection conditions may cause injury due to an operating error, or damage the system. When performing an inspection, always follow the diagnostic procedure. • Active bonnet control module falsely detects that there is no active bonnet sensor (left) setting
POSSIBLE CAUSE | • Active bonnet control module malfunction

Diagnostic Procedure

Action
Replace the active bonnet control module. (See ACTIVE BONNET CONTROL MODULE REMOVAL/INSTALLATION.)