VEHICLE SPEED SENSOR (VSS) INSPECTION [SJ6A-EL]

id051311252600

  Caution
  • Water or foreign material entering the connector can cause poor connections or corrosion. Be sure that water or foreign material do not enter the connector when disconnecting it.

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the tunnel member component.

4. Remove the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

5. Remove the insulator.

amxzzw00000196

6. Mark the manual shaft lever component as shown in the figure.

e5u513zw5007

7. Separate the manual shaft lever component from selector lever.

8. Disconnect the VSS connector.

amxzzw00000197

  Caution
  • Do not apply a shock in the VSS.
  • Do not damage the terminals.

9. Measure the resistance between the VSS terminals.

amxzzw00000198

  • If there is any malfunction, replace the VSS. (See VEHICLE SPEED SENSOR (VSS) REMOVAL/INSTALLATION [SJ6A-EL].)

  VSS resistance

  560—680 ohm

10. Connect the VSS connector.

11. Align the mark of the manual shaft lever component as shown in the figure.

e5u513zw5007

12. Install the manual shaft lever component installation nut.

  Tightening torque

  10.8—14.7 N·m {111—149 kgf·cm, 96.4—129.3 in·lbf}

13. Install the insulator.

  Tightening torque

  8—11 N·m {82—112 kgf·cm, 72—97 in·lbf}

14. Install the middle pipe. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L8, LF].)

15. Install the tunnel member component.

16. Connect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

17. Install the battery cover.