ELECTRICAL FAN CONTROL OUTLINE [L8, LF]

id0140i7103800

• Through cooling of the radiator and condenser by operation of the cooling fan according to vehicle conditions, engine reliability and cooling performance have been improved.
• The electrical fan control includes the regular-driving cooling function and the after-cooling function.
• The regular-driving cooling function operates according to the engine conditions during the engine operation.
• The after-cooling function operates when the vehicle has stopped at high engine temperature (ignition switch off).
• After the ignition switch is turned off, a main relay on request is sent to operate the after-cooling function. (See MAIN RELAY CONTROL OPERATION [L8, LF].)