MAIN RELAY CONTROL OPERATION [L8, LF]

id0140i7112000

• When the ignition switch is turned to the ON position, the main relay turns on and power is supplied to sensors and devices.
• When the ignition switch is turned from on to off, a main relay on command signal is received the main relay turns on and the following actions take place:

  1. Throttle valve control: Fully closed throttle learning function (See DRIVE-BY-WIRE CONTROL OPERATION [L8, LF].)
  2. After-cooling function of the electrical fan control (See ELECTRICAL FAN CONTROL OPERATION [L8, LF].)

• When the on request signal from the controls stop, the main relay turns off.