DOOR PAD REMOVAL/INSTALLATION

id091100620700

1. Disconnect the negative battery cable.(See BATTERY REMOVAL/INSTALLATION [L8, LF].)

2. Remove the following parts:

  (1) Door trim (See DOOR TRIM REMOVAL/INSTALLATION.)

  (2) Door speaker (See DOOR SPEAKER REMOVAL/INSTALLATION.)

  (3) Door module panel (See DOOR MODULE PANEL REMOVAL/INSTALLATION.)

3. Remove the fasteners.

amxzzw00000217

4. Remove the door pad.

5. Install in the reverse order of removal.