AUTO-DIMMING MIRROR REMOVAL/INSTALLATION

id091200099900

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See \nBATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the screw.

amxzzw00002732

4. Remove the auto-dimming mirror in the direction of arrow (1) shown in the figure.

ac5wzw00002992

5. Detach tabs while push the cover No.2 in the direction of the arrow (2) shown in the figure, then remove the cover No.2 in the direction of the arrow (3).

ac5wzw00002993

6. Disconnect the auto-dimming mirror connector.

ac5wzw00002994

7. Remove the auto-dimming mirror in the direction of arrow (4) from the mirror base.

ac5wzw00002995

8. Install in the reverse order of removal.