OIL PRESSURE SWITCH INSPECTION

id092200495300

1. Turn the ignition switch to the ON position and verify that the oil pressure gauge reading indicates L or below.

2. Start the engine and verify that the oil pressure gauge operates.

  • If the oil pressure gauge does not operate, inspect the related wiring harness.
    ― If the related wiring harness is normal, inspect the oil pressure. (See OIL PRESSURE INSPECTION [L8, LF].)
      • If the oil pressure is normal, replace the oil pressure switch.