EXTRACTOR CHAMBER REMOVAL/INSTALLATION

id091600449500

1. Remove the battery cover.

2. Disconnect the negative battery cable. (See BATTERY REMOVAL/INSTALLATION [L8, LF].)

3. Remove the rear combination light. (See REAR COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove clip A using a fastener remover and then remove the extractor chamber from the body.

e5u916zw5035

5. Install in the reverse order of removal.