DRIVELINE/AXLE TECHNICAL DATA

id035000800100

Item | Specification
--- | ---
Maximum front wheel bearing play | 0.05 mm {0.002 in}
Maximum rear wheel bearing play | 0.05 mm {0.002 in}
Rear drive shaft standard length | Left side: 778.5—788.5 mm {30.65—31.04 in} Right side: 818.5—828.5 mm {32.22—32.62 in}
Differential oil | Grade: API service GL-5 Viscosity: SAE 90 Capacity (approx. quantity): 0.6—0.8 L {0.63— 0.85 US qt, 0.53—0.70 Imp qt}
Backlash of pinion gear and side gear | 0.1 mm {0.004 in} or less
Differential pinion height | 0.038 mm {0.0015 in} or less
Drive pinion preload | 1.3—1.8 N·m {14—18 kgf·cm, 12—15 in·lbf}
Backlash of drive pinion and ring gear | Standard: 0.09—0.11 mm {0.0035—0.0043 in} Minimum value: 0.05 mm {0.0020 in} or more Variance: 0.07 mm {0.0028 in} or less
Ring gear preload | 0.49—2.45 N·m {5.0—24.9 kgf·cm, 4.4—21.6 in·lbf}
Maximum runout | 0.6 mm {0.024 in}
Initial torque (Reference value) | 0.29—0.98 N·m {3.0—10 kgf·cm, 2.7—8.6 in·lbf}