STARTING PROCEDURE FOR ON-BOARD DIAGNOSTIC TEST MODE [AUDIO]

id0902f6855500

  Note
  • All DTCs displayed in the on-board diagnostic test mode should be entered in the Audio Repair Order Form.

1. Turn the ignition switch to the ACC or ON position.

2. Turn the audio unit power to OFF.

3. While pressing the POWER/VOLUME switch, simultaneously press the AUX switch and the RPT/PRESET switch 4 for 2 s or more.

With RDS (radio data system)

amxzzw00002452

Without RDS (radio data system)

amxzzw00002453

  Note
  • If several DTCs are in the memory, they can be displayed using the SEEK/TRACK switch (up or down).

4. To stop the on-board diagnostic test mode, turn the ignition switch to the LOCK position.