COWL GRILLE REMOVAL/INSTALLATION

id091600444000

1. Remove the wiper arm and blade. (See WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove the covers.

e5u916zw5001

3. Remove the screws.

4. Remove windshield washer hose from cowl grille.

5. Remove the weatherstrip.

6. Pull the cowl grille in the direction of arrow (1) so that it is free from the pins, pull tabs A in the direction of arrow (2), and then remove the windshield.

7. Remove the cowl grille.

8. Install in the reverse order of removal.