POWER RETRACTABLE HARDTOP WARNING ALARM CONSTRUCTION/OPERATION

id092200110300

System Wiring Diagram

amxzzn00000498

Operation

Operation start sound

  • A buzzer in the instrument cluster sounds if both of the following two conditions are met:
    ― Power retractable hardtop operation conditions are met.
    ― The power retractable hardtop (open/close) switch is pressed.

Operation complete sound

  • A buzzer sounds when the power retractable hardtop open or close operation is completed.

Operation reject sound

  • A buzzer in the instrument cluster sounds if any of the following conditions are met:
    ― The power retractable hardtop operation conditions are not met when the power retractable hardtop (open/close) switch is pressed.
    ― The power retractable hardtop (open/close) switch is pressed with the power retractable hardtop system DTC detected.
    ― The power retractable hardtop (open/close) switch is pressed when the power retractable hardtop is fully closed and the system DTC is stored.
    ― Power retractable hardtop operation conditions are not met during power retractable hardtop operation.
    ― An power retractable hardtop system DTC is detected during power retractable hardtop operation.

  Warning
  • A buzzer in the instrument cluster sounds if any of the following conditions are met with the power retractable hardtop half open.
    ― Vehicle speed signal is input.
    ― The selector lever is in any position except P or N (AT vehicles).
    ― The selector lever is not in neutral (neutral switch normal condition) (MT vehicles).