ROOF/DECK PANEL MOTOR CONSTRUCTION

id091600101800

• Consists of a motor, connector, and gear.
• Two hall effect switches are located in the connector.
• In the connector, the roof panel motor has one hall effect switch and the deck panel motor has two (only one hall effect switch is used). (The hall effect switch does not detect rotation direction.)
• Hall effect switch 1 outputs one pulse cycle for each rotation of the motor axle and the power retractable hardtop control module detects motor rotation speed from this.

Roof Panel Motor Construction View

amxzzn00000609

Deck Panel Motor Construction View

amxzzn00000610