WHEEL UNIT ID REGISTRATION

id021200800400

  Note
  • After the wheel unit replacement, registration of the wheel unit identification codes must be performed.
  • ID registration can be done using the M-MDS, or not using the M-MDS.
  • Use the IDS (laptop PC) because the PDS (Plcket PC) does not support the wheel unit ID registration and monitoring wheel unit ID.

Using M-MDS

1. Connect the M-MDS to DLC-2.

amxzzw00000604

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • This function is available for only the IDS (notebook PC).
    1. Select the “Body”.
    2. Select the “TPMS Functions”.
    3. Select the “Wheel Unit ID Registration”.

3. Select an item from the screen menu.

  ― Wheel unit ID registration: WU ID Registration
  ― Monitoring wheel unit ID: Monitor WU ID Registration

4. Leave the vehicle with the ignition to off for 15 min or more.

5. Turn the ignition switch to the ON position.

6. Verify that the TPMS warning light turns on and off in 0.5 s cycles repeatedly.

7. Drive the vehicle at a speed of 25 km/h {15.5 mph} or more for 10 min to implement the wheel unit ID registration.

  Note
  • If the ID registration is not completed even after driving the vehicle for 10 min or more at a speed of 25 km/h {15.5 mph} or more, the TPMS warning light flashes.

8. Verify that the TPMS warning light turns off.

  Note
  • If the wheel unit ID registration cannot be performed after driving 10 min or more, refer to the symptom troubleshooting procedure.

Without Using M-MDS

1. Turn the ignition switch to the ON, then turn it off.

2. Leave the vehicle with the engine off for 15 min or more.

3. Drive the vehicle at a speed of 25 km/h {15.5 mph} or more for 10 min or more.

4. After driving for 10 min, verify that the TPMS warning light does not flash and is not illuminated.