CLOCK SPRING ADJUSTMENT

id081000802100

  Note
  • The adjustment procedure is also specified on the caution label of the clock spring.

1. Set the front tires straight-ahead.

  Caution
  • The clock spring will break if over-wound. Do not forcibly turn the clock spring.

2. Turn the clock spring clockwise until it stops.

amxzzw00001836

3. From the stopped position, turn the clock spring counterclockwise 2 3/4 turns.

amxzzw00001837

4. Align the mark on the clock spring with the mark on the outer housing.

amxzzw00001838